TROVIS-VIEW Software

Uniform interface for configuration and operation of various smart SAMSON devices



SYSTEM REQUIREMENTS for TROVIS-VIEW 4

  HARDWARE (minimum):
    - PC with Pentium processor or equivalent (1 GHz or faster), at least 512 MB RAM
    - Serial RS-232 interface or USB interface (with USB to RS-232 adapter or USB Converter 3 
      for TROVIS 5500 Automation System)
      Plus suitable hardware depending on SAMSON device used
    - 1 GB for x86 and 2 GB for x64 of free disk space (includes installation of Microsoft® 
      .NET Framework 4.0)

  SOFTWARE:
    - Operating system: WINDOWS® XP, WINDOWS® Vista, Windows® 7, Windows® 8 and 8.1
      Installation requires administrator privileges.
    - Microsoft® .NET Framework 4.0
    - Web browser: Microsoft® Internet Explorer® (version 6.0 or higher) or equivalent
    - PDF reader



INSTALLATION

  Insert the CD-ROM and installation will start automatically. If this is not the case, open 
  the SETUP.EXE file from the CD-ROM.

  Select the components to be installed.

  Depending on the type of connection used between PC and device (USB), additional drivers may 
  have to be installed. Suitable drivers are contained on the CD-ROM or they can be downloaded 
  from the SAMSON website at www.samson.de in the Services / Software section.

  For further information on operating the devices, go to the ? menu in TROVIS-VIEW. Additional 
  information is also contained in the INFO and TOOLS folders on the CD-ROM.



SOFTWARE UPDATES

  Updated versions of TROVIS-VIEW will become available as we are constantly developing the software 
  further. The latest version of TROVIS-VIEW can always be downloaded from the SAMSON website at 
  www.samson.de in the Services / Software section.



USER LEVELS AND PASSWORDS

  In TROVIS-VIEW, user rights are managed in password-protected user levels (Device menu, User Level). 
  Select a user level and enter the associated password, if applicable. This prevents device data 
  from being changed unintentionally or without authorization. The following list contains all user 
  levels and the associated passwords. The passwords are also contained in the mounting and operating 
  instructions of the devices. Passwords are case sensitive.

  Device	User level		Password

  3374		Maintenance technician	-
		Expert			samson
		Factory calibration	samson

  3730-2	Specialist		-

  3730-3	Specialist		-
	
  3730-4	Specialist		-

  3730-5	Specialist		-

  3730-6	Specialist		-

  3731-3	Specialist		-

  3731-5	Specialist		-

  3780		Specialist		-

  3785		Specialist		-

  3787		Specialist		-

  Media 6	Maintenance staff	-
		Flow rate		DURCHFLUSS (up to TROVIS-VIEW V3.20)
		Specialist		samson (TROVIS-VIEW V3.21 and higher)
		Basic calibration		GRUNDABGLEICH

  5431		Customer		-

  5432		Customer		-

  5433		Customer		-

  5575		Customer		-
		5575-0011		5575-0011	(TROVIS 5575-0011)

  5576		Customer		-

  5579		Customer		-

  5724/5725	Customer		-
		Specialist		samson

  5757		Customer		-
		Specialist		samson

  5757-7	Customer		-
		Specialist		samson

  5824/5825	Customer		-
		Specialist		samson

  5857		Customer		-
		Specialist		samson

  6493		Maintenance technician	-

  6495-2	Maintenance technician	-



SAMSON AG does not assume any liability for damage caused by using this software.
Some designations, logos and brand names used on the CD-ROM are patented, 
registered or protected trademarks.



=======================================================
SAMSON AG, MESS- UND REGELTECHNIK
Weismüllerstraße 3
60314 Frankfurt am Main, Germany
www.samson.de

=======================================================
Microsoft, Internet Explorer, and Windows are registered trademarks of Microsoft Corporation 
in the United States and/or other countries.

=======================================================
en 2013-11 ABu
