This DTM is for the SAMSON FF Positioner 3730-5 device revision 2 (Firmware R1.52 K2.00-2.09)

DTM revision: V.1.0.0.6


------------------
Hints for the DTM:
------------------

- Writing all parameters to the device: because some parameters can only be written into the device if the corresponding
block mode is in O/S, all blocks have to be set in mode O/S before writing these parameters.
After writing of the parameters, the old modes can be written into the device.

Recommended procedure for writing all parameters to the device:

1.) with the button 'Set all target modes to 'Out of Service O/S'' set all block modes in O/S
2.) write the parameters into the device
3.) with the button 'Restore all target modes' set all blocks to the old modes


- Option leakage detection: in the directory 'Diagnosis - Leakage detection' only a subset of the parameters were supported.
  No graphs were supported.

- FST: parameter 'Delay time after step' is not supported

